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4MP AI-ISP Fixed Bullet Network Camera
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Key Features

· High quality imaging with 4MP resolution
· AI-ISP for excellent noise reduction effect
· 24/7 colorful imaging via AI-ISP technology
· High quality imaging with 4MP resolution, 1/1.8" CMOS sensor and F1.0 large aperture lens
· Efficient H.265+ compression technology
· Clear imaging against strong backlight due to 120 dB WDR technology
· Focus on human and vehicle targets classification
· Water and dust resistant (IP67)
· Built-in microphone for real-time audio security

Dimensions
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Specification

	Camera

	Image Sensor
	1/1.8" Progressive Scan CMOS Sensor

	Min. Illumination
	Color: 0.0005 Lux @ (F1.0, AGC ON) ,0 Lux with Warm light on

	Illumination Distance
	30m (warm light)

	Smart IR
	N/A

	Pan/Tilt/Rotation Range
	Pan: 0° ~ 360°
Tilt: 0° ~ 90°
Rotation: 0° ~ 360°

	Lens

	Focal Length
	2.8/3.6 mm

	Aperture
	F1.0

	FOV
	2.8 mm @ F1.0 Horizontal FOV: 110°, Vertical FOV: 59°, Diagonal FOV: 130°
3.6 mm @ F1.0 Horizontal FOV: 95°, Vertical FOV: 51°, Diagonal FOV: 113°

	Lens Mount
	M16

	DORI

	DORI
	2.8 mm @ F1.0, D: 57 m, O: 23 m, R: 11 m, I: 6m
3.6 mm @ F1.0, D: 68 m, O:  27m, R:  14m, I:  7m

	Compression Standard

	Video Compression
	H.264/H.264+/H.265/H.265+/MJPEG

	H.264 Codec Profile
	Base/Main/High profile

	H.265 Codec Profile
	Main Profile

	Video Bit Rate
	11 Kbps ~ 10Mbps

	Triple Streams
	Support

	Audio Compression
	G.711A, G.711U

	Audio Bit Rate
	64 Kbps

	Image

	Max. Image Resolution
	4M (2688 × 1520)

	Main Stream
	50Hz: 20fps 4M (2688 × 1520)
25fps 4M (2560 × 1440)
25fps 1080P (1920 × 1080)
60Hz: 20fps 4M (2688 × 1520)
30fps 4M (2560 × 1440)
30fps 1080P (1920 × 1080)

	Sub Stream
	50Hz: 25fps 720P (1280 × 720)
25fps D1 (704 × 576) ,25fps CIF(352 × 288)
60Hz: 30fps 720P (1280 × 720)
30fps D1 (704 × 480) , 30fps CIF (352 × 240)

	Third Stream
	50Hz:25fps CIF (352 × 288)
60Hz: 30fps CIF (352 × 240 )

	Image Setting
	Brightness/Contrast/Saturation/Hue/Sharpness

	Shutter Time
	Auto/Manual, 1/3 ~ 1/100000s

	Day/Night
	IR Cut Filter

	Wide Dynamic Range
	120dB

	Digital Noise Reduction
	2D/3D DNR

	BLC
	Support

	HLC
	Support

	ROI
	Support

	Rotate
	Support

	Smart Feature

	Basic Event
	Motion detection, video tampering

	Smart Event
	Smart motion detection, line crossing, intrusion, region entrance, region exiting (support alarm triggering by specified target types (human and vehicle) )

	Face Detection
	N/A

	Network

	Network Storage
	NAS (NFS, SMB/CIFS)

	Protocols
	TCP/IP, ICMP, HTTP, HTTPS, FTP, DHCP, DNS, DDNS, RTP, RTSP, RTCP, NTP, IGMP, UPnP, SMTP, UPnP-TM, Cloud

	System Compatibility
	Onvif (Profile S, Profile G, T) , SDK

	Security
	HTTPS encryption, IP address filter, basic and digest authentication for HTTP/HTTPS, TLS 1.1/1.2, WSSE and digest authentication for Open Network Video Interface

	User
	Up to 40 users

	Web Browsers
	Plug-in required live view: IE 10, IE 11
Local service: Chrome 57.0+, Firefox 52.0+

	Mobile Surveillance
	IOS, Android

	Active Deterrence

	Red/Blue Light Warning
	N/A

	Sound Warning
	N/A

	Interface

	Communication Interface
	1 RJ45 10 M/100 M self-adaptive Ethernet port

	On-board Storage
	Up to 256GB

	MIC
	Support

	Speaker
	N/A

	Audio I/O
	N/A

	Alarm I/O
	N/A

	Reset Button
	Support

	General

	Operating Conditions
	(-40°C ~ 60°C) (-40°F ~ 140°F)
Humidity 95% or less (non-condensing)

	Power Supply
	DC12V ± 25%

	POE
	PoE (802.3 af)

	Power Consumption
	MAX. 8W

	Protection Level
	IP67

	Material
	Metal

	Dimensions
	Φ76 × 215.8 mm

	Gross Weight
	900 g




Accessory
Optional
	AC-JB02
	AC-PM03
	AC-CMB02
	AC-PC06
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Installation Methods
	Junction Box
	Pendant Mounting
	Vertical Pole Mounting
	Corner Mounting
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	IPC4BF2R4+JB02
	IPC4BF2R4+JB02+CMB02
	IPC4BF2R4+PM03
	IPC4BF2R4+JB02+PC06



[image: ]
image3.png
4MP




image4.png
LVAR:]

-
-
e
1/1.8" Large Sensor





image5.png




image6.png
F1.0 Large Aperture





image7.png
Smart Motion
Detection





image8.png
Y

Built-in Mic





image9.png
IP67




image10.png
215.8mm(8.50")

$76.0mm(2.99") 127.7mm(5.03")
3-(4.5mm(0.18"
| = @64. 0mn (2. 52")
) é ,

13 ”
= S — ~_@74.5m(2.92")

~ %

=1





image11.png




image12.png
'

e

P




image13.jpeg




image14.png




image15.png




image16.png




image17.png




image18.png




image1.png




image2.png




image19.png
Homax




image20.jpeg
Homaxi Inc. www.homaxi.com





